Assignment 3

Dionne Pasion

200344266

Part 1

1. Measuring air flow per unit of time through a tube, called an air flow meter.
2. Measuring position, velocity, orientation of the sensor called a accelerometer  
   Sources: <https://www.elprocus.com/types-analog-digital-sensors/>

Part 2

1. Most likely the maximum raw reading of the senor has been reached
2. y = 1204x-0.59

Part 3

As a mercury tilt switch relies on the mercury moving over a certain point to determine the supposed temperature at that point if it is pre tilted by physical location then it will get to that point at a lower temperature instead of the actual temperature if the sensor is on a flat surface.